

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Activity: Use of Jigsaw | | Location: New Theatre | | Date: September 2013 |
| Hazards: **List what could cause harm from the activity** | Who could be Harmed: **List who might be harmed from this activity** | Control Measures in Place: **For each hazard list the measures you will be taking to minimise the risk identified** | Risk Rating  **With Control Measures in place what is the risk rating (see table below)** | Further Actions: **is there anything else that needs to be reduce risk further** |
| **Electric Shock** | **Users** | * **Machine will be PAT tested annually** * **Operators should visually check machine and cable before use for cracks to casing and cable damage** * **Cable to be routed away from the moving parts of the machine** * **Fitted with RCD protection if used outside workshop** | **Low** |  |
| **Dust, splinter** | **Users/ others in immediate area** | * **Goggles and gloves (if desired) to be worn when using the equipment** * **Use local extraction when possible** | **Low** |  |
| **Electric Hand Tool** | **Users/ others in immediate area** | * **Operator will ensure that there is plenty of room to move comfortably around the material being worked on and that the material is firmly clamped** * **Those helping a user must also wear PPE and stay far away or behind saw to prevent accidental injury** | **Low** |  |
| **Sharp Objects, Severe Cuts, Entanglement in Equipment** | **Users** | * **Blades to be inserted and used following the manufacturer’s guidelines** * **Use a blade designed for material being cut** * **Users instructed to cut away from body** * **Jigsaw must be unplugged when changing blades** * **User must not wear baggy clothing, loose jewellery, and must tie back long hair** | **Low** |  |
| **Damaged/Faulty Equipment** | **Users** | * **Equipment will be checked before each use visually to ensure there are no defects in casing, or blade** * **Damaged equipment not to be used and reported to workshop manger** | **Low** |  |
| **Working at Height** | **Users/ others in immediate area** | * **All work at height should follow work at height risk assessment** | **Medium** |  |
| **Physical Fatigue** | **Users** | * **Regular breaks advised** | **Low** |  |